[Textinfo]
0#Cancel
1#Done...
2#Timeout
3#Wait for response
4#No Com Connection...
5#Wait for end of Transmision
6#Find...
7#Send RS232 FAIL: Port not open
8#No Ports found.
9#Port is already open...
10#Open last COM
11#Error by opening Com Port
12#To Login: Password is in Clipboard, Username: flir
13#Recived Answer
14#Connection Test Fail
15#Downloading...
16#Start Download...
17#No File found.
18#Remove
19#Picture stored
20#No Picture to save...Start Videoconnection...
21#Connected
22#Connect with Telnet...
23#Find COM Ports...
24#already exist.\r\nSould the new be insertet at the End of File?
25#Save as TXT
26#stored.\r\nInserted sings
27#Open
28#Close
29#wait...
30#Start
31#Measure...
32#Grab all Measurement Data
33#Starting...
34#No Camera
35#no Cam found
36#Temperatur
37#Seconds
38#Could not open File:
39#Clear all Treeview contend... really do that?
40#Clear Tree
41#No Control, you software is not unlocked.
42#No Control...no License found in settings.txt
43#No Control...License Fail
44#Control enabled...License Pass
45#Too much resisted Telnet Users. Restart your Camera...
46#Set reference for Value A first...
47#Set reference for Value B first...
48#Set Fusion Window:
49#Set Isotherm:
50#Program is already running
51#This program is already running now.\r\nShould all other instances of this program being closed?\r\n\r\nActual parallel running : 
52#No foldes found.
53#No files found.
54#Read Folders...
55#Starting connection to Camera...
56#Index~Day~Time~Size~Filename~Info
57#Size check FAIL
58#File not found
59#Deleting
60#deleted
61#Choose program
62#Start the selected file to try it working?
63#Video file could not been created. Select a video codec first.
64#already exist. Overwrite?

[Controls]
btn_abbruch#Cancel
TP_flir_control#Control
group_language#Sprache/Language
btn_SetLanguage#OK
groupBox10#Buttons
chk_F_UseTastaturForControl#Use Keypad to Control
label1#Q     R\r\n    W\r\nA  E D\r\n    S\r\n           F
btn_flir_bt8#Save
label45#!MSD:
btn_flir_bt5#Menu
btn_flir_bt4#R
btn_flir_bt3#L
btn_flir_bt2#Down
btn_flir_bt1#Up
btn_flir_bt6#Back
btn_flir_bt0#Play
btn_F_002_Nuc#NUC (Calibration)
label_F_StatusVideo#Video only with USB mode containig "UVC"
btn_F_CamFind#Search...
TP_view1#View 1
groupBox19#Palette
groupBox3#Isotherm
label11#Filtercolor:
label12#Value:
groupBox18#Freeze
btn_F_001_FreezeOff#OFF
btn_F_000_FreezeOn#ON
TP_view2#View 2
groupBox28#Level and Span
btn_F_011_ModeMan#Manuell
btn_F_010_ModeAuto#Auto
label31#Backlight (%)
label42#MSX offset:\r\n(focus position)
TP_setMeas#Measurement
label55#Messfequenz (max. 10.6)
group_SetMeas#Set Measure by Mouseclick
chk_F_SetMeasVerify#Check Settings (takes time, is safer)
chk_F_SetRemoveAll#turn all off
chk_F_SetSpot5#Spot 5
chk_F_SetSpot4#Spot 4
chk_F_SetSpot3#Spot 3
chk_F_SetSpot2#Spot 2
chk_F_SetBox4#Box 4
chk_F_SetBox3#Box 3
chk_F_SetBox2#Box 2
chk_F_SetBox1#Box 1
chk_F_SetSpot1#Spot 1
chk_F_008_AdvMeasMenu#advancedMeasureMenu
btn_F_012_ReadSpot#Read Spot1 
btn_F_009_ReadBatt#Read Batt
TP_Setup1#Setup 1
groupBox32#Filter: Row / Colum
label47#Row:\r\nThres\r\nThresPix\r\n\r\nColum:\r\nThres\r\nThresPix
chk_F_004_row#Enable Row
chk_F_005_column#Enable Colum
groupBox31#Filter: apr3x3
label46#Killnumber:\r\nlamda:\r\nthresholdInit:\r\nthresholdMax:
chk_F_003_apr3x3Enable#Enable
groupBox34#Filter: temporal
label49#Level (0-16): Thres (0-24):
chk_F_007_Temporal#Enable
groupBox33#Noise Gen
label48#Level (0-255):
chk_F_006_Noisegen#Enable
groupBox30#Filter: bilateral
label44#Sigma (0-500):
chk_F_002_BilatEnable#Enable
TP_Setup2#Setup 2
groupBox40#.image.fusion
label54#xpanVal\r\nypanVal\r\nzoomFactor
groupBox38#...histRect
btn_F_013_HistoRectSet#Set
label53#set_x1\r\nset_x2\r\nset_y1\r\nset_y2
groupBox37#contadj.colDistr
label52#filterParam\r\nlinearPercent\r\nplateauPercent
groupBox36#contadj
label51#brightness\r\ncontrast\r\nfrequency
groupBox35#contadj.autoAdj
label50#TSpanMin\r\nTSpanMinAuto\r\nfilterParam
TP_Setup3#Setup 3
groupBox24#Special
chk_F_010_RemDeathPixel#remove death Pixel
groupBox2#Parameter
label3#Emissionsgrad:\r\nRel Luftfeuchte:\r\nReflekt. Temp:
groupBox1#USB Modus
groupBox41#Nuc
btn_F_017_NucCommit#Trigger
label56#FramesLog2:
chk_F_012_AutoNuc#Enable Auto NUC
chk_F_009_NucShutter#Shutter
TP_IRVideo#IR-Video
groupBox15#Download (USB: RNDIS)
btn_ftp_SequenzOpenFolder#open folder
btn_ftp_SequenzDownload#Download
btn_ftp_SequenzGetFileSize#Get Filesize
txt_ftp_SequenzDownloadFile#default.seq
groupBox42#Thermal Record
btn_f_IRVid_GetSettings#get Settings
label57#Count (Frames):\r\nFrequency:
btn_F_020_IRVid_Store#Store
btn_F_019_IRVid_Stop#Stop
btn_F_018_IRVid_Start#Start
chk_F_011_RTAction#on: Record\r\noff: Playback
label58#Filename:
btn_F_CamDevice#Start
propertyGrid1#PropertyGrid
groupBox20#Digital Zoom
btn_F_006_Zoom8#x8
btn_F_016_ChanVisual#Visual
btn_F_005_Zoom4#x4
btn_F_004_Zoom2#x2
btn_F_015_ChanFusion#MSX
btn_F_014_ChanIR#IR
btn_F_003_Zoom1#x1
group_Screenshot#Screenshot (Video)
btn_F_Scrennshot#Save
btn_F_ScrennshotFolder#open folder
groupBox21#Power Control
btn_F_008_Restart#Restart
btn_F_007_Standby#Standby
TP_flir_Control2#Measurement
btn_F_graphstop#Stop
btn_F_graphstart#Start
btn_F_graphClear#delete all Points
label30#Timeout (Sec):
btn_F_Graphsave#Save all measurment data to text file
groupBox22#Measure
TP_M_Graph#Graph and Measurements
chk_f_Grap_B4_Avr#Box 4 Avr
chk_f_Grap_B4_Min#Box 4 Min
chk_f_Grap_B4_Max#Box 4 Max
chk_f_Grap_B3_Avr#Box 3 Avr
chk_f_Grap_B3_Min#Box 3 Min
chk_f_Grap_B3_Max#Box 3 Max
btn_F_GrabMeas#Grab all Measurement Data
chk_f_Grap_B2_Avr#Box 2 Avr
chk_f_Grap_B2_Min#Box 2 Min
chk_f_Grap_B2_Max#Box 2 Max
chk_f_Grap_B1_Avr#Box 1 Avr
chk_f_Grap_B1_Min#Box 1 Min
chk_f_Grap_B1_Max#Box 1 Max
chk_f_Grap_S5#Spot 5
chk_f_Grap_S4#Spot 4
chk_f_Grap_S1#Spot 1
chk_f_Grap_S3#Spot 3
chk_f_Grap_S2#Spot 2
groupBox8#Settings
label_F_punkte#0
label_F_ItemColor#Mausklick: Set Color
chk_F_CurveTitelVisible#Visible
label26#Titel:
radio_F_mbox#MBox (Area)
radio_F_Spot#Spot (Point)
chk_F_CurveVisible#Visible
label29#Curve:
TP_flir_Terminal#Terminal
tabPage2#Send / Control
groupBox17#Timeouts
label13#Telnet:\r\nUART:
chk_rs232_FlirResponseOutput#Print Flirresponse
txt_rs232_lastCom#COM38
BTN_RS232_Oenlast#Open last:
btn_rs232_refresh#Refresh Ports
BTN_RS232_Clear#Clear
label10#Textbox:
TXT_Send_B#0 127 128 129 255
BTN_RS232_Save#Save
TXT_Send_S_2#.services.net.interface.RNDISFN1
TXT_Send_S_1#.image.sysimg.measureFuncs.spot.5.active true
TXT_Send_S_0#usbfn RNDIS
BTN_RS232_Open#Open
label4#Text:
label9#Bytes:
label2#Rset:
label7#Rls:
tabPage3#Setup
CHK_RS232_NotOnTop#Print not ever on TOP
label_DSR#DSR
CHK_RS232_Sonderzeichen#Sonderzeichen darstellen
btn_rs232_DTR#DTR
CHK_RS232_ToBytes_time#Zeit im Bytefenster mitschreiben
btn_rs232_RTS#RTS
CHK_RS232_UseStartByte#Startbyte:
label_CTS#CTS
label_CD#CD
CHK_RS232_ToBytes#Text in Bytes wandeln und darstellen
CHK_RS232_SendChar13#CR (char 13) am ende
label8#Normal (und aktuell markiertes):
label6#Farbe Empfangen:
CHK_txt_WriteTime#Zeit mitschreiben
label5#Farbe Senden:
TP_flir_Tree#Tree
txt_tree_filename#TreeData.txt
groupBox16#Cameraresponse
btn_tree_getFullResponse#Get full Response
txt_tree_set#true
btn_tree_set#Set
btn_tree_load#Load Tree
btn_tree_save#Save Tree
txt_tree_grabnode#.
btn_tree_GrabNode#Grab Node
TP_flir_web#Web
group_web_webcam#Direct Webcam
groupBox23#Init
btn_web_webcam#Webcam
btn_web_pixkill#Pixel Replacement
btn_web_ServiceStart#Service Startseite
tbtn_web_webcam#Direct\r\nWebcam
btn_web_startseite#192.168.0.2
txt_web_pw#3vlig
txt_web_user#flir
TP_flir_Hid#HID
groupBox7#Recive HID
label_HID_key1#Key1
groupBox5#Verbindungs Log
groupBox6#Send HID (DEC: 0 - 255 oder HEX: 0x00 - 0xff)
txt_usb_send#1 1
groupBox9#µC Serial
btn_hid_uart1Rx_del#DEL
chk_FLIR_auswerten#Auswerten
txt_hid_uart1Tx#rset .image.flow.digitalFilter.noiseGen.enabled false
groupBox4#HID
txt_usb_VendorID#0483
txt_usb_ProductID#0004
btn_use_Uart#use UART
btn_usb_finddevice#use HID
label_F_Status#Status...
btn_FLIR_ConnTelnet#Telnet
btn_tree_GrabNode#Readout
btn_tree_set#Set
btn_tree_save#Save Tree
btn_tree_load#Load Tree
groupBox16#Response from Camera
btn_tree_getFullResponse#Read with extra Info
group_telnetIP#Telnet IP
group_license#Enter License
group_diff#Difference (Value A - Value B)
radio_diff_all#all Measurements
radio_diff_NurAktive#only active
btn_F_setDiff#Set
btn_F_021_diffOff#OFF
groupBox43#IR Window (Picture In Picture)
chk_f_SetPipWindow#Set IR Window
btn_f_SetPipFullscreen#IR full Screen
label11#Color:
label12#Value A:
label21#Value B:
label27#View:
radio_iso_Mode1#below value A
radio_iso_Mode2#above value A
radio_iso_Mode3#between A and B
chk_iso_SendToCam#Send changes to Camera immediately
btn_iso_SetAll#Send all
groupBox44#Picture folder from the camera (USB: RNDIS)
btn_pic_GetFolders#List folders
btn_pic_DeleteFolder#delete selected
btn_pic_NewFolder#New:
btn_pic_ListFiles#List all images from Camera
btn_pic_SetActiveFolder#All new images to this folder in Camera
btn_F_026_ResetPicCount#Picture counter to 0 (next image: FLIR0001)
groupBox45#Interval (time lapse)
label28#Store next image in:
group_DownloadPictures#Download images from Camera
btn_pic_Download#Download all and delete them from Camera
chk_pic_DownOverrideIfExist#Override if exist
btn_pic_DownOpenFolder#Open folder
TP_M_AuswertungA#Analysis A
TP_M_AuswertungB#Analysis B
chk_M_AActive#Active A
groupBox27#monitored measurement
groupBox26#condition to perform
radio_M_Aover#above
radio_M_Aunder#below
radio_M_Agleich#equal
radio_M_Abetween#betweeen
label34#threshold 1:
label35#threshold 2:
groupBox46#action after trigger
chk_M_AMakePicture#Camera takes picture
chk_M_ARun#run always:
chk_M_ARun2#run single:
chk_M_ATurnOff#turn off:
radio_M_ATurnoffAuswert#Analysis A
radio_M_ATurnoffMeas#Measurement + Analysis
chk_M_BActive#Active B
groupBox48#monitored measurement
groupBox49#condition to perform
radio_M_Bover#above
radio_M_Bunder#below
radio_M_Bgleich#equal
radio_M_Bbetween#betweeen
label33#threshold 1:
label39#threshold 2:
groupBox47#action after trigger
chk_M_BMakePicture#Camera takes picture
chk_M_BRun#run always:
chk_M_BRun2#run single:
chk_M_BTurnOff#turn off:
radio_M_BTurnoffAuswert#Analysis B
radio_M_BTurnoffMeas#Measurement + Analysis
TP_Pictures#Pictures
groupBox51#Videocodec
btn_mov_create#create
btn_mov_store#save and close
groupBox52#video path and file name
btn_mov_openfolder#open\r\nfolder
groupBox53#Recording
chk_mov_rec#REC
btn_mov_grabFrame#Grab single frame
label36#MM:SS (frames):
groupBox54#Interval (time lapse)
btn_mov_raffStart#Start
btn_mov_raffStop#Stop
TP_Movie#Movie
TP_ImgProc#Imageprocessing
groupBox56#sharpen
radio_IP_Sharp1#low
radio_IP_Sharp2#middle
radio_IP_Sharp3#high
groupBox55#difference/subtraction
radio_IP_Diff1#Diff
radio_IP_Diff2#Subst.
chk_IP_GrabRefpic#G E T
groupBox57#averaging
chk_IP_Sharpen#ON
chk_IP_Substract#ON
chk_IP_Avr#ON
chk_IP_ColDiff#ON
btn_IP_SetColDiff#Set
groupBox58#Color difference
radio_IP_ColDiff_Typ1#Solid (Base: Gray)
radio_IP_ColDiff_Typ2#gradations (Base: Black)

[conmenu]
btn_GrabNodesLevel1#Grab with level 1 Subnodes
btn_GrabNodesAllLevel#Grab with all Subnodes
tbtn_RemoveSubnode#Remove all Subnodes
tbtn_RemoveALLSubnodes#Remove tree content
tbtn_ReadSpot#Read Spot
tbtn_ReadMbox#Read MBox
tbtn_f_RefDiff1#Read Diff 1
refreshTabelle#Refresh View
tbtn_KillMeasurement#Kill Measurement
tbtn_F_removeAll#Turn all Offline
tbtn_f_GrabAllMeasData#Grab all Measurement data
tbtn_pic_DownSelected#Download only selected
tbtn_pic_DownAll#Download all
tbtn_pic_DelSelected#Delete selected from Camera
tbtn_pic_DelAll#Delete all from Camera